Power is off
STANDBY
Com Vol
-
Psh Sq
VOL
COM
888.888
STBY
888.888
Audio
Panel
Intercom
MIC
Split
1
2
MON
1/PA
1
2
DTK
187°
Field2
GS
138KT
DIS
98.6NM
DIS
98.6NM
DIS
98.6NM
XPDR
ID
IDENT
1200
ON
R
VOL
NAV
888.888
STBY
888.888
Visual
NORTH UP
50NM
DTK
187°
Field2
GS
138KT
DIS
98.6NM
Configure User Fields
OBS
358°
FROMF
GOMDA
NEXTN
88.01NM
8.01NM
o
o
o
o
Flight
Plan
Pan Mode
Waypoint Info
Next
Map Menu
Map Overlays
TOPO
Terrain
Traffic
NEXRAD
Airspaces
Airports
Intersections
VORs
NDBs
Constraints
TRACK UP
Fields
Change
Fields
Restore
Defaults
Highlight
Map
Detail
Most
Least
Traffic
HDG UP
12NM
6NM
Terrain
HDG UP
12NM
6NM
GSL
1800FT
Terrain
FT
-500
-1000
-1500
Terrain Menu
View
360°
Arc
Layers
Flight
Plan
Legend
TAWS
TAWS
Inhibit
Test TAWS
Altitude
GSL
AGL
Charts Menu
Night view
Provider
Navigraph
Brightness
5
Please reload your charts after switching day/night view
______ / ______
ALT
DTK
DIS
APT Info
Enroute
APT Info
APT Info
Add Enroute Waypoint
Waypoint Options
Activate Leg
Insert
Before
Insert
After
Along
Track
Hold At
Waypoint
Load
Airway
Load Sar
Waypoint Info
Remove
VNAV Options
Waypoint: GILRA
Along Track
0 NM
Type
At
3000 FT
1000 FT
Revert
Constraint
Remove
Constraint
VNAV
Departure Options
Select Departure
Remove Departure
Arrival Options
Select Arrival
Remove Arrival
Approach Options
Activate Approach
Frequency
109.90
Activate
Vectors to Final
Activate
Missed Approach
Select Approach
Remove Approach
Airway Options
Collapse All
Airways
Select Airway
Remove Airway
Search & Rescue Options
Collapse Search
Pattern
Select Pattern
Remove Pattern
Hold Options
Activate Hold
Insert After
Edit Hold
Exit Hold
Remove
Select Import
Used:
Empty:
DepartureDestinationDISESA
Route Options
Activate
Invert
& Activate
Preview
Edit
Copy
Delete
Departure
Arrival
Approach
Activate
Approach
Activate
Vectors
To Final
Activate
Missed
Approach
Public
DIS:
88.0NM
BRG:
358°
Info
Preview
Procedures
Runways
Location

Elevation
124FT
Time Zone
UTC_
Fuel
Avgas/Jet

View Charts
Runway
Lighting
Traffic

Weather data
NOT AVAILABLE
NOTAMS
NOT AVAILABLE
NRST VRPs
NOT AVAILABLE
Frequencies
WX Data
NOTAMs
NRST VRPs
DIS:
88.0NM
BRG:
358°
Location
Caen
FRANCE
Nearest VOR
CAN
2.6NM
309°
DIS:
88.0NM
BRG:
358°
Used WPTs
11
View List
Edit
Delete
DIS:
88.0NM
BRG:
358°
Location
Caen
FRANCE
Frequency
114.45
Nearest Airport
2.6NM
309°
VOR Class:
Station Declination:
DIS:
88.0NM
BRG:
358°
Location
Caen
FRANCE
Frequency
404
Nearest Airport
2.6NM
309°
Marker Description:
User identifier
USR00
Airport
Comment
N49 W0
Position Type
Rad / Dist
Latitude / longitude
N 49°06.81'
W000°27.37'
REF WPT
LFRK
Radial
181.6°
Distance
5.6NM
Temporary
Elevation
_____ FT
Create
Import
Copy
Paste
Load
Used Waypoints: 0 / 100
Bank
Bank 1
Bank Name
Delete All
Radar
STAB:
ON
Tilt
0.00°
Show
Tilt
Show
BRG
Bearing
0°
Mode
Weather
Scan
Horizontal
Gain
Calibrated
Airspace
Status
Target ALT
1000FT
Altitude Type
MSL
VS Profile
500FPM
Offset
1NM
Before
Target Waypoint
Status
Begin Descent in 00:29:45
VS Required
-845FPM
Restore Defaults
Display Messages
Active VNAV Constraint
IMJUS
5800FT
4800FT
VS Target
-484 FPM
Flight Path Angle
-3.00°
VS Required
-480 FPM
Time to TOD
08:58
Vertical Deviation
25 FT
VNAV Enabled
P.POS
From
______
To
______
Flight Plan
Active FPL
Leg
P.POS -> LFRN
Use Sensor Data
Mode
Flight Plan
FOR PLANNING PURPOSES ONLY
Fuel on Board
_____GAL
Fuel Flow
_____GAL/HR
Ground Speed
_____KT
Prev
_____
(Cum)
_____
Next
Fuel Req to LFRNN
_____GAL
Fuel at LFRNN
_____GAL
Reserve at LFRNN
__:__:__
Range
__._NM
Efficiency
_____NM/GAL
Endurance
__:__:__
Select Leg
Fuel planning Menu
Fuel Type
AVGAS
Unit
Gallons
FOR PLANNING PURPOSES ONLY
Indicated ALT
0FT
BARO
__.__IN
Use Sensor Data
CAS
___KT
TAT
___°C
TRK
___°
HDG
___°
Ground Speed
0KT
Density ALT
_____FT
TAS
___KT
Wind Direction
___°
Wind Speed
___KT
Head Wind
___KT
DALT/TAS/Winds Menu
Baro Unit
mb
Magnetic/True
Controller
Frequency
Filter
None
In Range
Update
ATC Menu
Source
VATSIM
Auto Update
Max Distance
None
Direction
Up
Start
Preset
00:00:00
Preset
Timer
Generic Timer
-00:00:00
Criteria
Power On
Reset
Timer
Trip Timer
00:00:00
Criteria
Power On
Reset
Time
Departure Time
LCL
Checklist Menu
Group
Emergency Checklists
Checklist
Icing
Clear Current Checklist
Clear All Checklists
Select Group
Select Checklist
Utilities - Map Menu
View
Map
Scale
1
Auto center
Select Map
888
888
A
R
M
AP
888
888
A
R
M
∆
P
T
∆
88.888
ALERT
FPM
FT
HPA
IN HG
UP
DN
AP
FD
YD
GA
LVL
VNV
ARM
HDG
NAV
APR
REV
ALT
VS
FLC
Alt
Sel
Use
Aircraft
Altitude
Selector
HDG
345°
CRS
345°
OBS
345°
Baro
1013mb
HDG SYNC
DTK SYNC
TO/GA
Baro STD
Utilities - Autopilot Menu
Alt Sel 100/10
Baro Unit
mb
Alt Presel
Auto Arm
Logs Menu
Group
Group name
Section
Section name
Reload
Select Group
Select Section
SCREEN CLEANING MODE
Press the HOME key to exit.
Version Info
Software Version:
License type:
WTT Mode:
COM/NAV index:
Database
Source:
Version:
Backlight
5
Mitigation
Medium
Touch the buttons above to configure the user fields
Restore Defaults
COM Channel Spacing
8.33 kHz
License Information
Enter License
Check License
Activate License
Deactivate License
Clear License
Information
Metars are provided by the avwx online service.
You should open an account on https://avwx.rest
Then get a free token api and report it here.
You must be connected to internet for Metars to work. Metar are significant only while playing with live weather.
Your avwx token:
Enter Token
Test Metar
Information
Charts are provided by the Navigraph service.
You must have a valid Navigraph account for charts.
Use the "Connect Navigraph" button to connect.
You'll need your mobile phone or tablet with a QrCode reader and your Navigraph Credentials.
Status: Connected
Connect Navigraph
- Scan the QrCode and follow the link
- Or type the url below in your browser
- Enter Credentials and verification code
- Wait 5 seconds
Traffic data
Traffic refresh
Medium
Traffic on ground
Messaging system
Airspace messages
Approach auto activation
Direct To button in map
Keyboard
QWERTY
Disable Click Sound
Target Altitude Source
Autopilot
Allow Com/Nav switch
Wind on ground
Map compass
Display GSI in Map
Map HDG line
Map Runway lines
None
Track Vector Length
Off
Map Traffic Range
10
Map VOR Rings
Bush Trip Flight Plan
Map icon
Propeller
Map Fuel Ring
Fuel Reserve Time
45
Map Visual Button
Never
Visual Distance
10
Map fields pages
1
Optimize Map FPS
Safe Taxi
XPDR VFR Default
1200
Fuel Type
AVGAS
Fuel Unit
Gallons
XPDR + Audio Panels
XPDR + Audio
DTK Auto Sync
Extended Vol Knob
Flight Planner ID
VCALC
VNAV Indicator
Aircraft Type
GA
SDK Version
Restart GPS
Safe taxi settings
Enable
Max Speed
30
Zoom Level
2
Import / Export
Export
Import
Import local file
Import from PMS50
Delete
Select Checklist
Pilot ID
_____
Waypoint Identifier
Find
Backspace
Fast Find
______
No suggestion
1
2
3
4
5
6
7
8
9
0
Q
W
E
R
T
Y
U
I
O
P
A
S
D
F
G
H
J
K
L
Z
X
C
V
B
N
M
Space
Recent
Nearest
Flight Plan
User
Search Name
Search City
Select Nearest List
Find
COM Standby
117.95
Backspace
1
2
3
4
5
6
7
8
9
Monitor
0
XFER
Recent
Nearest
Flight Plan
User
Select Nearest List
Select Frequency
Select Frequency
XPDR
0123
Backspace
0
1
2
3
4
5
6
7
VFR
Mode
Standby
On
Altitude Reporting
Audio Panel
Split Mode
Playback
Controls
Cabin
Speaker
Speaker
Volume
3D Audio
Monitored Radios
MIC Selection
COM 1
COM 1
COM 2
COM 2
NAV 1
NAV 2
DME
ADF
1
2
3
4
5
6
7
8
9
0
Q
W
E
R
T
Y
U
I
O
P
A
S
D
F
G
H
J
K
L
.
Z
X
C
V
B
N
M
-
ABC/abc
Space
Backspace
VS Profile
Backspace
1
2
3
4
5
6
7
8
9
.
0
+-
Mode
Before
After
VS Profile
Backspace
1
2
3
4
5
6
7
8
9
0
Format
D°M.M'
Waypoint Coordinates
S 89°56.98'
W000°27.83'
N
S
E
W
1
2
3
4
5
6
7
8
9
0
LAT
Duplicate Waypoints
Search Results for ""
PROC - Departure
Sequence
Airport
Departure
Runway
Transition
Load Departure
PROC - Arrival
Sequence
Airport
Arrival
Transition
Runway
Load Arrival
PROC - Approach
Sequence
Airport
Approach
Transition
Channel / ID
_____ _____
Load Approach
Load Approach
& Activate
Load Airway
Sequence
Entry Waypoint
Airway
Exit Waypoint
Load
Hold At Waypoint
Direction
Course
Direction
Turn
Leg Length
Leg Type
Leg Time
Load Hold
Search and Rescue Patterns
Initial Waypoint
USR000
SAR Pattern
Exp. Square
Initial Track
360°
Initial Turn Direction
Left
Leg Length
15.0NM
Track Spacing
1.0NM
Leg Count
10
Load Pattern
Load Pattern
& Activate
Select SAR PAttern
Direct To
Waypoint
FPL
NRST APT
Select Waypoint
Bearing:
294°
Distance:
366NM
Position:
N 48°04.32'
W001°43.93'
Course To
___°
Hold
___°
SAR
___
Messages
Select User Field
Data
Function
Page
Flight Plan Preview
Sequence
Activate
Sort Alpha
Popup Message
OK
Working Message
OK
User Waypoints - All
User Waypoints Menu
Bank
Bank 1
Bank Name
Delete All
But1
MSG
But2
But3
But4
Enter
Left
Right
50NM