***************************************************************************************************************
* This file defines optional GTN750 custom tile maps to be displayed in the Utility Map page
* This is an example and you should customize and rename it to "custom_map_layers.txt".
* The file must be named "custom_map_layers.txt" and must be put into the Config/pms50-gtn750 package folder
* BE CAREFUL to save the file somewhere outside the package when you update the GTN750 version.
***************************************************************************************************************

***************
* MAP section *
***************
* All entries are mandatory
* name is the internal map name id. It must be unique across this file.
* provider is the map provider.
* displayShortName is the name displayed in the utility map page menu.
* displayLongName is the name displayed for map selection.
* minZoom is the minimal zoom value (minimum is 1).
* maxZoom is the maximal zoom value (maximum is 19).
* url is the tile server url.
******************************************************************************************************************************************

* Tile servers examples: https://wiki.openstreetmap.org/wiki/Raster_tile_providers

[MAP]
name=osm
provider=OpenStreetMap
displayShortName=STREET
displayLongName=Open Street Map
minZoom=2
maxZoom=19
url=https://tile.openstreetmap.org/{z}/{x}/{y}.png

[MAP]
name=otm
provider=OpenTopoMap
displayShortName=TOPO
displayLongName=Open Topo Map
minZoom=2
maxZoom=19
url=https://tile.opentopomap.org/{z}/{x}/{y}.png
